|  |  |  |  |
| --- | --- | --- | --- |
|  | Bus Frequency | Blocking Delay Time | Freqency |
| Baseline | 8 MHz | 100 ms | 5 Hz |
| Expected | 20 MHz | 40 ms | 25 Hz |
| Measured With AD2 | 20 MHz | 40 ms | 25 Hz |
| Expected | 24 MHz | 33.3ms | 30 Hz |
| Measured With AD2 | 24 MHz | 35.7ms | 28 Hz |