|  |  |  |  |
| --- | --- | --- | --- |
|  | Bus Frequency | Blocking Delay Time | Freqency |
| Baseline | 8 MHz | 100 ms | 5 Hz |
| Expected | 20 MHz | 40 ms | 12.5 Hz |
| Measured With AD2 | 20 MHz | 40 ms | 12.5 Hz |
| Expected | 24 MHz | 33.3 ms | 15 Hz |
| Measured With AD2 | 24 MHz | 33.3 ms | 15 Hz |